# ID 20816

Coordinate for homing is out of data format.
Description | When using the axis referencing command G74, the value of a coordinate is out of the permissible numerical range. The individual coordinate values of the axes specify the order of the homing axes.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the value of the coordinate.
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016)
%2: | Error value [-]
%3: | Lower limit value [-]
%4: | Upper limit value [-]
Error type | 1, Error message from NC program.