# ID 120268

Change of spline type not permitted while spline interpolation is active.
Description | The spline type cannot be changed while Akima or B spline interpolation is active. For more information on spline functions, see [PROG// Section: Akima spline interpolation] .[PROG// Section: B spline interpolation].
Response | Class | 2 | Program abort.
Solution | Class | 6 | Before changing spline type in CNC program, deactivate spline function.
Error type | 1, Error message from NC program.