# ID 50619

The velocity of the conveyor belt exceeds the axis' maximum feedrate.
Description | The velocity CONV_VEL specified in the #SYNC IN command exceeds the maximum velocity of the axis parallel to the conveyor belt.
Response | Class | 6 | Movement stop.
Solution | Class | - |
Parameter | %1: | Logical axis number [-]
Number of the axis in the conveyor belt’s direction
%2: | Current value [0.1 µm/s]
Programmed conveyor belt velocity
%3: | Upper limit value [0.1 µm/s]
Maximum velocity of the belt axis in G1 blocks
Error type | -