# ID 110288

Changing the hardware counter id requires restart of the control.
Description | The parameter P-AXIS-00042 indicating the unique hardware identification of the counter cannot be changed while the CNC kernel is running. The new hardware identification is not transferred; the previous active hardware identification remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Change the entry P-AXIS-00042 only in configuration mode or when the CNC is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value of P-AXIS-00042.
%3: | Corrected value [-]
Corrected value of P-AXIS-00042.
Error type | 2, Error message on data transfer of parameter lists to controller.