# ID 150088

Number of handwheels does not match with the number of logical handwheels.
Description | When interpreting the manual mode parameters, the system detects that there are more or less handwheel parameter data records than specified in the parameter P-MANU-00001.
Response | Class | 3 | Manual mode parameters are not adopted in the CNC, but the CNC start-up is continued using default parameters.
Solution | Class | 6 | Correct value for parameter P-MANU-00001 or Add missing handwheel parameter data records or remove surplus records.
Parameter | %1: | Current value [-]
Value of parameter P-MANU-00001 in manual mode parameter data record.
%2: | Expected value [-]
During interpretation of manual mode parameters, handwheel parameter records were found.
Error type | 2, Error message on data transfer of parameter lists to controller.