# ID 21057

Too many parameters in signal command programmed.
Description | The maximum number of permissible parameters when waiting for a signal (#WAIT) or sending a signal (#SIGNAL) has been exceeded.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Modification of NC program.
Parameter | %1: | Limit value [-]
Maximum permissible number of parameters
Error type | 1, Error message from NC program.