# Distance from corner (P-CHAN-00012)

P-CHAN-00012 | Distance from corner for speed limit look ahead
Description | The logical signal SLD 1 ->0 is generated depending on the parameters 'distance from corner' or 'time from corner'. Here, corner means the position in the block at which the speed rises again above the speed limit.
Parameter | speed_limit_look_ahead.dist_from_corner
Data type | UNS32
Data range | 0 ... MAX(UNS32)
Dimension | 0.1µm or µs
Default value | 0
Remarks |