# ID 40008

Error occurred while copying PLC version string to HLI.
Description | A PLC application that uses PLC libraries containing function blocks according to the PLCopen specifications to solve function blocks must call exactly one instance of the MCV_PlatformBase function block. During the initialisation phase of the Motion Control Platform, the utility FB MCV_ChkLCsHLIVer is called within the FB MCV_PlatformBase, with which the version ID of the HLI interface on the PLC side is transferred to the Motion Controller for checking.

The utility FB notifies the error message if the PLC fails to provide its HLI version identifier to the motion controller because the copy version identifier on the HLI was aborted with an error.

At the output "ErrorID" of the FB MCV_PlatformBase this error message is made available for the PLC application.

Response | Class | - | The FB MCV_PlatformBase sets sets its “Error” output to TRUE and the “Done” output to FALSE.
Solution | Class | - | Reset and logout the PLC application. Retransmit and start the PLC application during PLC runtime. If the error occurs again, contact the control supplier.
Error type | -