# ID 110229

Logical axis number in compensation value list and in start-up list not equal.
Description | A logical axis is to use a compensation value list. This is why this compensation value list is interpreted. The system detects that the number of the logical axis of the compensation value list does not match the number of the logical axis that is to use this list.
Response | Class | 3 | Abort interpretation of the compensation value list.
Solution | Class | 7 | Check which compensation value list is to be used for the axis. Possibly change change the number of the logical axis in the list or use a different list.
Parameter | %1: | Current value [-]
Number of a logical axis. This number (P-COMP-00001) comes from the compensation value list that was to be used.
%2: | Expected value [-]
Number of the logical axis to be used by the compensation value list (P-STUP-00036).
Error type | -