# ID 120615

M/H functions with synchronisation type MNS_SNS with and without path-related pre-output in the same NC block not possible.
Description | M and H functions with synchronisation type MNS_SNS with and without path-related pre-output are not possible in the same NC block. Either N/H functions with or without path-related pre-output may be used in an NC line.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the NC program.
Error type | 1, Error message from NC program.1, Error message from NC program.