# ID 90011

Block memory for non-relevant channel blocks engaged.
Description | Non-relevant blocks are blocks without motion data for the TRC. M functions are an example of non-relevant blocks: The number of consecutive non-relevant channel blocks is greater than the internal block memory allocated.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Modify the NC program. Interrupt the sequence of non-relevant channel blocks by a block with motion data.
Parameter | %1: | Upper limit value [-]
Number of the possible non-relevant blocks in sequence.
Error type | 1, Error message from NC program.