# ID 70528

Volumetric Compensation: axis could not be compensated because it is not homed.
Description | An axis that is part of a Volumetric Compensation is about to receive a correction value but the axis is not homed yet.
Response | Class | 3 |
Solution | Class | 6 | Reset CNC, home axis
Parameter | %1: | ID of Volumetric Compensation
%2: | logical axis number
Error type | 11, Error message from position controller.