# ID 110524

Modulo range exceeds data range because of resolution settings.
Description | Modulo range defined through the parameters P-AXIS-00127 and P-AXIS-00126 was exceeded. This is caused by a change in distance resolution. This is set via parameters P-AXIS-00234 and P-AXIS-00233.
Response | Class | 3 | None
Solution | Class | 7 | Check and modify the modulo limits and the parameters of distance resolution.
Parameter | %1: | Logical axis number [-]
Log. axis number P-AXIS-00016
%2: | Current value [-]
P-AXIS-00126
%3: | Limit value [-]
Maximum possible value for P-AXIS-00126 with constant distance resolution
%4: | Current value [-]
P-AXIS-00127
%5: | Limit value [-]
Minimum possible value for P-AXIS-00127 with constant distance resolution
Error type | 2, Error message on data transfer of parameter lists to controller.