# ID 20889

Channel parameters: Face-ID is out of range of permissible values.
Description | During start-up, the entry for the facing ID is checked for the valid value range. The value of the Face-ID P-CHAN-00008 in the channel parameters list is out of range.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | Check and modify the value of the Face-ID P-CHAN-00008 in the channel parameters before the next controller start-up. During start-up in case of conflict the value of Face-ID is set to the maximum limit.
Parameter | %1: | Error value [-]
Invalid value of Face-ID in channel parameter list
%2: | Upper limit value [-]
Maximal value of Face-ID
%3: | Corrected value [-]
Automatically corrected value of Face ID
Error type | 2, Error message by data transfer from parameter list into control device.