# ID 90178

Illegal combination of parameters in multipath configuration.
Description | The parameters for using single or multi path configurations are incorrect in the start-up list and the channel parameter list. In the channel parameter list the parameter multi_path_configuration 0 # Enable 2-path programming (P-CHAN-00261) is incorrectly set for the use of multipath configurations.

Correct setting for multipath configuration:

Channel parameter list:

multi_path_configuration 1 # Enable 2-path programming (P-CHAN-00261)

Activate the function:

configuration.tool_radius_comp.function MULTI_PATH # P-CHAN-00550

Alternatively, the function can be activated in the start-up list:

configuration.channel[0].tool_radius_comp.function MULTI_PATH # P-STUP-00080

Correct setting for single path configuration (default):

Delete both parameters in each of the lists.

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Correct the parameters concerned in the channel parameter list (or start-up list.)
Error type | 1, Error message from NC program.