# ID 140036

Error while writing a drive telegram.
Description | An error occurred while writing the drive telegram in the drive. Possible reasons are:

- An error occurred during the transmission of the idents.
- An invalid value for ident 15 (telegram type) was written.
- A value which cannot be transferred cyclically is entered in the configuration list of the drive telegram (ID 16) (see ID 187, list of configurable data in drive telegram).
- A value which cannot be transferred cyclically is entered in the configuration list of the master data telegram (ID 24) (see ID 188, list of configurable data in MDT).

Response | Class | 1 | Warning output
Solution | Class | 1 | Correction of the invalid values
Parameter | %1: |
Logical axis number (P-AXIS-00016).
%2: |
Ident when the error occurred.
Error type | -