# ID 13431

For the variable V.P.Sys_Probes_in_spindle only 0 or 1 permitted.
Description | For the variable V.P.Sys_Probes_in_spindle a wrong value is entered, only 0 or 1 are permitted.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Define the variable V.P.Sys_Probes_in_spindle in the NC program SysMeasWcsConfig.nc.
Error type | 1, Error message from the NC program