# ID 110568

Change of P-AXIS-00363 requires restart of the control.
Description | An attempt was made to change the axis parameter list entry P-AXIS-00363 by updating the axis parameter list but the ALLOW_RESOLUTION_CHANGE bit in P-AXIS-00015 is not set. Since a change of P-AXIS-00363 changes the resolution of the axis, this change is rejected and a restart of the controller is required.
Response | Class | 0 | Warning output, changed value is not adopted.
Solution | Class | 0 | Restart of the controller with changed parameter P-AXIS-00363
Parameter | %1: |
Axis number
%2: |
Incorrect value
%3: |
Corrected value
Error type | -