# ID 21385

Impermissible use of a cycle spindle name.
Description | This error output is caused by using a cycle spindle name (@X..) in the main program, or by a direct call of a cycle as a stand-alone program. A cycle spindle name may only be used in the cycle program itself (e.g. @S=1000). Example with error:

N05 X0 Y0 Z0 G00

N20 G01 X200 F500

N25 @S=1000 M3

N40 L CYCLE [NAME=dummy1.cyc …]

N50 G01 Y300 F1000

N60 G01 Z300 F2000

N90 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. . Only use cycle spindle name in the cycle. Start cycle only by a global sub program call within the main program (L CYCLE [...]).
Parameter | %1: | Current value [-]
Error type | 1, Error message from NC program.