# Static offset (P-AXIS-00073)

P-AXIS-00073 | Static offset between master and slave axes
Description | Static difference between the master and slave axes in the event of differences between the master and slave axes. The offset sign results from the calculation instruction: OFFSET = SLAVE - MASTER
Parameter | kenngr.gantry_offset
Data type | SGN32
Data range | MIN(SGN32) < gantry_offset < MAX(UNS3
Axis types | T, R
Dimension | T: 0.1 µm | R: 0.0001°
Default value | 0
Drive types | ----
Remarks |