# ID 120626

Tracking axis on main axis index.
Description | The axis for tangential tracking tangential tracking P-CHAN-00095 is on a main axis index. See also [PROG// Section: Automatic axis tracking (C axis tracking)]
Response | Class | 2 | Abort NC program
Solution | Class | 6 | Check configuration, only tracking axis with axis index > 2 allowed.
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned axis P-AXIS-00016.
%2: | Current value [-]
Axis index of the tracking axis.
Error type | 1, Error message from NC program.