# ID 110391

Second entry for adjustment of position controller proportional gain was specified as 0.
Description | The second proportional gain P-AXIS-00247 of the dynamic kv adjustment was specified as 0. This is an invalid value.
Response | Class | 1 | Value is initialised with default value.
Solution | Class | 1 | Correct parameter list of axis.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00247
%3: | Corrected value [-]
P-AXIS-00247
Error type | 2, Error message on data transfer of parameter lists to controller.