# ID 21799

The configured count of GCM-Nodes is less than zero.
Description | The amount of the in the list configured GCM-Nodes is less than zero (nil).
Response | Class | 2 | Reset of the NC channel.
Solution | Class | 3 | Increase the value of the GCM-Node count so that it is greater than zero (nil).
Parameter | %1: | Error value [-]
Current, incorrect value.
Error type | 1, Error message from NC program.