# ID 51087

During active orbit extension NC commands with position initialisation are not permitted.
Description | As soon as the command #TRACK CHAN ON [EXTEND …] was evaluated in a channel configured as an orbit channel, the orbiting process becomes active. Afterwards, no NC commands requiring an initialisation of the NC channel with axis positions may be used if the radius in the down channel is > 0.
NC commands requiring a channel initialisation include, for example, #CS, #TRAFO and #CHANNEL INIT.

Response | Class | 4 | Abort NC program processing.
Solution | Class | 6 | Check and modify the NC program in the orbit channel.
Parameter | %1: | Current value [0.1 10^-3 mm or ø]
Current radius in the orbit channel.
Error type | -