# ID 130125

PDU receiver not announced or unknown.
Description | The receiver specified in the message is not known to the controller or has not yet been registered.. The message is undeliverable and ignored. Possible error cause is the programming of an unknown receiver by explicit programming of the receiver ID in command #MSG.
Response | Class | 3 |
Solution | Class | 1 | Check the programmed receiver in the #MSG command and correct the receiver. Only the documented receivers are possible.
Parameter | %1: | Current value [-]
%2: | Incorrect value [-]
%3: | Current value [-]
%4: | Current value [-]
%5: | Current value [-]
Error type | 3, Error message from communication.