# ID 110379

torq_detect_torque_limit greater than 1000.
Description | The value of torq_detect_torque_limit is greater than 1000, i.e. it is greater than 100%.
Response | Class | 1 | Warning output. The value of torq_detect_torque_limit is set to 1000 (100%) automatically.
Solution | Class | 1 | Choose value of torq_move_torque_limit less or equal than 1000 (100%).
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [0,1%]
Current value of torq_detect_torque_limit.
%3: | Limit value [0,1%]
1000 (100%)
%4: | Corrected value [0,1%]
Corrected value of torq_detect_torque_limit.
Error type | 2, Error message by data transfer from parameter list into control device.