# ID 110401

Illegal measurement method. Only one method may be selected.
Description | Invalid parameter setting for P-AXIS-00117 was assigned to the measurement. The parameter P-AXIS-00117 is assigned the default value.
Response | Class | 1 | None.
Solution | Class | 1 | Only use parameter P-AXIS-00117 if P-AXIS-00115 is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number of axis affected P-AXIS-00016.
%2: | Current value [-]
Current parameter P-AXIS-00269.
%3: | Current value [-]
Current parameter P-AXIS-00117.
%4: | Corrected value [-]
Corrected parameter P-AXIS-00117.
Error type | 2, Error message on data transfer of parameter lists to controller.