# Including a contour rotation (P-CHAN-00215)

P-CHAN-00215 | Including a contour rotation in the tracking axis
Description | For a contour rotated in the plane with #ROTATION ON[], the rotation angle about the Z axis is not included in the tracking axis. If this is required, this parameter activates the inclusion of the rotational offset in the calculation. This function is only useful if automatic tracking (P-CHAN-00101) is inactive for technological reasons.
Parameter | consider_rot_tracking_offset
Data type | BOOLEAN
Data range | 0: Contour rotation (#ROTATION) is not included in the tracking axis (default). 1: Contour rotation (#ROTATION) is included in the tracking axis.
Dimension | ----
Default value | 0
Remarks |