# Position controller trace (TraceType 3):

Data | Value |
all data | 0x000000 | All data is logged.
m_sollw_absolut | 0x000001 | Absolute metric set position.
m_istw_absolut | 0x000002 | Absolute metric actual position.
active_feedrate | 0x000004 | Currently set velocity.
active_accel | 0x000008 | Currently set acceleration.
cmd_pos_outp (INTIME only) | 0x000010 | Absolute set position output to the drive interface.