# Defining the type of logged events (P-STUP-00043)

P-STUP-00043 | Defining the type of logged events
Description | The CNC offers the options of filing events in a history memory (logging entries). The parameter permits the user-specific definition of CNC logging entries to be logged. Depending on troubleshooting or the analysis requirement, event logging can be filtered in order to reduce the number of entries to be logged or analysed right from the outset.
Parameter | configuration.position_controller.log_level
Data type | UNS32
Data range | 0 ... MAX(UNS32)
Dimension | ----
Default value | 0
Remarks |