# Refreshing tool data (#TOOL REFRESH)

Following command is provided for the repeated inclusion of tool data of the active tool, e.g. in additional axes after an axis exchange:

Syntax:
#TOOL REFRESH | Refresh data of active tool

The command results in the immediate inclusion of the already available data of the active tool. No more tool data is adopted from an internal tool list [5] or requested from an external tool management function. The D word reprogramming function can be deselected.