# ID 120285

Axis exchange while active spline interpolation.
Description | With active Akima or B-Spline interpolation, no axis exchange is allowed. For more information on spline function, see [PROG// Section: Akima spline interpolation]. [PROG// Section: B spline interpolation].
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Deactivate the spline function before releasing or requesting axes in the CNC program.
Error type | 1, Error message from NC program.