# Path type (P-CHAN-00403)

P-CHAN-00403 | Type of path of a program path
Description | This parameter defines the type of the program path bit-encoded. A path specification may also be used for several path types.
Parameter | path[i].type
Data type | UNS16
Data range | 0x01 (main program path) 0x02 (subroutine path) 0x04 (path for #MSG SAVE) 0x08 (path for storing debug data *.dbg) Combinations:
0x03 (main prog.+ subroutine path)
0x05 (main prog. path + path for #MSG SAVE)
0x06 (subroutine path + path for #MSG SAVE)
0x07 (main prog. + subroutine path + path for #MSG SAVE)
0x0B (main prog. path + subroutine path + path for debug data)
0x0F (main prog. path + subroutine path + path for #MSG SAVE and debug data)

Dimension | ----
Default value | 0
Remarks | This parameter is available as of CNC Build V3.1.3052.05 and higher.