# ID 294510

KPS: Cabinet temperature too high PMx.
Description | The cabinet temperature is too high.
Response | Class | 7 | Ramp-down braking. All active commands inhibited.
Solution | Class | 6 | Check the function of the fans in the control cabinet. Check whether the ventilation openings on the cabinet are unimpeded and whether enough air is circulating. Reduce the ambient temperature. If necessary, choose a different installation site.
Error type | 11, Error message from position controller.