# ID 70499

Identifier for additional 'Ready for Power' test not configured in cyclic input process data.
Description | The input name set in P-AXIS-00711 was not found in the configured input process data of the drive. If the reference signal is transmitted in a real-time status bit of a SERCOS drive, enter the value "S-0-0135" in this parameter P-AXIS-00711. In this case the drive status word does not have to be set up explicitly in the drive process data because it is always transferred automatically.
Response | Class | 1 | Warning output, additional 'ready for power' test is disabled by assigning an empty string to P-AXIS-00711.
Solution | Class | 1 | Either change P-AXIS-00711 to a value configured in the process data of the drive, or extend the process data of the drive by the element entered in P-AXIS-00711.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [-]
Set value of P-AXIS-00711.
Error type | -