# ID 40081

FB error: error id 11 of FB STRING_TO_BUF.
Description | Function block calls the PLC runtime specific function block STRING_TO_BUF. This specific function block displays error code 11. For more information we point to help for *_TO_BUF function blocks and the specific help of function block STRING_TO_BUF of the PLC runtime supplier.
Response | Class | - | Character string at input "InputString" isn't copied to the byte array at output "ByteArray".
Solution | Class | - | Please contact your motion control supplier.
Error type | -