# ID 70320

Activation of plane compensation not possible, since compensation value table is invalid.
Description | Could not activate plane compensation since no compensation value table exists or it contains errors. See also: [FCT-C5// Section: Plane compensation] [COMP// Section: Plane compensation]
Response | Class | 7 | Stop of axis, plane compensation remains inactive
Solution | Class | 6 | Correct Compensation table see [COMP]
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
Error type | 11, Error message from position controller.