# ID 120405

Tool data are inconsistent.
Description | The specified tool geometry is not known. The geometry must be a ball end cutter or a shaft end cutter.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the tool geometry of the tool in the tool data list.
Parameter | %1: | Current value [-]
Tool number
%2: | Current value [0.1 µm or 0,0001°]
Tool radius
%3: | Current value [-]
Wrong tool geometry
%4: | Current value [0.1 µm or 0,0001°]
Internal state of tool geometry compensation
Error type | 1, Error message from NC program.