# ID 315012

Tv factor for distance control is out of permissible range.
Description | The D-Tv derivative action time for distance control [FCT-M3] may not be outside the limit values. Parameterisation is executed using:

- Description for axis-specific distance control
- Description for 3D distance control

Response | Class | 1 | Warning is output and correct the Tv factor.
Solution | Class | 1 | Check and correct the parameter for the Tv factor
Parameter | %1: | Logical axis number [-] or Logical channel number [-]
Logical axis number Axis parameters of the axis affected for axis-specific distance control, logical channel number Logical number of a NC channel (P-CHAN-00400) for 3D distance control.
%2: | Error value [-]
Incorrectly parameterised value of Tv factor
%3: | Lower limit value [-]
Minimum value of Tv factor
%4: | Upper limit value [-]
Maximum value of Tv factor
%5: | Corrected value [-]
Corrected value of Tv factor
Error type | -