# ID 20010

Programmed function requires at least one more axis.
Description | A previous axis release prevents this G-function from executing. Example circular interpolation: Wrong: N10 #PUT AX[X] N20 G02 R10 Y20 F200

Correct:

Solution (do NOT return axis):

…

N20 G02 R10 Y20 F200

...

Response | Class | 2 | Abort NC program processing. .
Solution | Class | 3 | Remove unhallowed axis release from NC-program code.
Error type | 1, Error message from NC program.