# ID 110504

Change of id axis specific current values transformation requires restart.
Description | An attempt was made to change the transformation id of the actual value transformation P-AXIS-00381 by updating the axis parameter list. This is not possible; a change requires a controller restart.
Response | Class | 0 | Warning output, the value of P-AXIS-00381 will not be changed.
Solution | Class | 0 | Change parameter and restart control.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis
%2: | Current value [-]
Changed value of P-AXIS-00381
%3: | Corrected value [-]
Old value of P-AXIS-00381
Error type | 2, Error message by data transfer from parameter list into control device.