# ID 21907

At least one main axis is missing for the function.
Description | At least one main axis is missing in order to use the function. Example with error: N240 G18 G1 Z15 X2 N250 #PUT AX [Z] N260 #ANG=30 X25

To use the #ANG command, both main axes of the active plane are required. In the given example, the Z axis is missing.

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the NC program.
Error type | 1, Error message from NC program.