# ID 150099

max_inkr_pro_takt is 0.
Description | The manual mode parameters are read and interpreted by the CNC. The program detects that the value 0 was specified in the manual mode parameters for one of the P-MANU-00007 parameters.
Response | Class | 3 | Manual mode parameters are not transferred to the CNC.
Solution | Class | 6 | Correction of the value for P-MANU-00007 so that it is > 0. Reinterpret manual mode parameters by restarting CNC System.
Parameter | %1: | Current value [-]
Value specified in the manual operation parameter set for P-MANU-00007.
%2: | Limit value [-]
Limit value that was exceeded.
%3: | Logical control element number [-]
Logical number of input device where the value of parameter P-MANU-00007 exceeds the limit value.
Error type | 2, Error message by data transfer from parameter list into control device.