# Programmed M01 stop during next forward movement (P-CHAN-00279)

P-CHAN-00279 | Programmed M01 stop during next forward movement
Description | Suppression of stop on next forward movement with M01.
Parameter | forward_backward.disable_m01_2nd_forward
Data type | BOOLEAN
Data range | 0: The process is also stopped in next forward direction with M01. 1: Stopping with M01 omitted in next forward direction.
Dimension | ----
Default value | 0
Remarks |