# Number of filter cycles to filter actual spindle speed (P-CHAN-00835)

P-CHAN-00835 | Number of filter cycles to filter actual spindle speed
Description | The actual spindle speed may be noisy under certain circumstances. To smooth the actual speed, this parameter can activate a filter. The parameter specifies the number of filter cycles that are used for smoothing.. The value 0 deactivates the filter.
Parameter | thread_cutting.n_cycles
Data type | UNS16
Data range | 0 <= n_cycles <= 25
Dimension | ---
Default value | 0
Remarks | P-CHAN-00835 only acts when thread cutting is active at the actual spindle speed. (Thread cutting with actual spindle speed (P-CHAN-00834)). Available as of V3.1.3080.17