# ID 110244

Logical axis number of master axis is missing for gantry operation.
Description | The axis is marked as a slave axis of a gantry combination in P-AXIS-00015 parameter, but there is a missing entry for the lead master axis P-AXIS-00070.
Response | Class | 3 | None.
Solution | Class | 7 | Use correct entry for logical axis number P-AXIS-00070 of lead master axis in the gantry combination.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Logical axis number [-]
Current logical axis number of the master axis P-AXIS-00070.
Error type | 2, Error message on data transfer of parameter lists to controller.