# ID 20180

Unknown spindle name or equal sign is missing.
Description | Either the spindle name programmed in NC block is unknown in NC channel (P-CHAN-00007, P-CHAN-00053) or, if the spindle name has more than one character, the equals sign is missing before the speed value . Example (assuming: Spindle name is „SPINDLE“):

Wrong:

N10 G00 X0 Y0 Z0

N20 SPDL=1000 M03

:

N1000 M30

or

N10 G00 X0 Y0 Z0

N20 SPINDLE1000 M03

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 SPINDLE=1000 M03

:

`N1000 M30`

Response | Class | 2 | Abort NC program processing..
Solution | Class | 3 | Check and modify NC program. Correct spindle name according to the configured name P-CHAN-00007 **. **Hint: Only the main spindle name P-CHAN-00053 may be used for the main spindle in the NC program.
Error type | 1, Error message from NC program.