# ID 120199

Change of coordinate system with active spline interpolation not possible.
Description | An active coordinate system cannot be changed or disabled when the spline function is active. Example of correct activation/deactivation: %spline_ks N05 #CS ON[0,0,0,0,0,30] N10 G151 X3 Y25

N20 X15 Y15

N30 X23 Y12

N40 X25 Y25

N50 X30 Y35

N60 G150 X50 Y37.5

N70 #CS OFF

N70 M30

For more information on spline functions, see
[PROG// Section: Akima spline interpolation].

Response | Class | 2 | Program abort.
Solution | Class | 6 | First deactivate spline function then change or deactivate the coordinate system.
Error type | 1, Error message from NC program.