# ID 90088

End of program with active contour masking process. (contour error).
Description | At the end of program contour masking process is still enabled.
Response | Class | 3 | Abort NC program processing.
Solution | Class | 6 | Modification of NC Program: Insert an additional motion block, this allows the contour masking process the calculation of an intersection point of the contour. Following the deselection of the contour masking and the tool radius compensation before the end of the program.
Parameter | %1: | Block number [-]
Error type | 1, Error message from NC program.