# ID 90133

The coordinate of the corrected point is outside of the permissible range.
Description | The tool radius compensation calculates coordinates of the equidistant path. The error occurs when the coordinate of the corrected circle centre point exceeds the permissible range of data format.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the NC program
Parameter | %1: | Error value [-]
Calculated coordinate
%2: | Lower limit value [-]
%3: | Upper limit value [-]
%4: | Block number [-]
Corresponding block number in NC program
%5: | Logical axis number [-]
Logical axis no.
Error type | 1, Error message from NC program.